**Specification RUSSIAN BLEND CRUDE OIL – REBCO**

***Specifications Corresponding to GOST TU 39-1623-93:***

|  |  |  |
| --- | --- | --- |
| Density API at 30 degrees | | C 0,870 |
| API Gravity | | 32.00 |
| Viscosity at 80 C, Max | | 16.0 |
| Flash Point (in locked cubicle) Max | | 35 C |
| Pressure of saturated pours under 38 C | | 38 C |
| kilopascal/mm mercury column | | 7/50 |
| Paraffin ( contents in % ) | | 6,0 % |
| Temperature of melting | | C - 49 |
|  | |  |
| **Contents** | | % |
| \* Sulphur | | 1.8 |
| \* Nitrogen | | 0.25 |
| \* Chamois -acid resins | | 0.9 |
| \* Asphatents | | 0.9 |
| Salt | | 100 mg / L |
| Coking % | | 2.06 |
| Ash % | | 0.004 |
|  | |  |
| **Distillation Vol. recovered** % | |  |
| 0 - 200°C | | 21.00 |
| 300°C | | 41.00 |
| 350°C | | 50.00 |
| Water and Sediments, Max | | 1.2 |
|  | |  |
| **REBCO (GOST 9965-76)** | | |
| Maximum Sulfur Content 1,8% Paraffin Content 6,0% Maximum Water & Sediment Content 1,2% Distillation, Weight 21% Up to 200° Ñ min 21 Up to 300° Ñ min 41 Up to 350° Ñ min 50 Maximum salts content, MG/L 100 | | |