**Specification RUSSIAN BLEND CRUDE OIL – REBCO**

***Specifications Corresponding to GOST TU 39-1623-93:***

|  |  |
| --- | --- |
| Density API at 30 degrees | C 0,870 |
| API Gravity | 32.00 |
| Viscosity at 80 C, Max | 16.0 |
| Flash Point (in locked cubicle) Max  | 35 C |
| Pressure of saturated pours under 38 C | 38 C |
| kilopascal/mm mercury column | 7/50 |
| Paraffin ( contents in % ) | 6,0 % |
| Temperature of melting | C - 49 |
|   |   |
| **Contents** | % |
| \* Sulphur | 1.8 |
| \* Nitrogen | 0.25 |
| \* Chamois -acid resins | 0.9 |
| \* Asphatents | 0.9 |
| Salt  | 100 mg / L |
| Coking % | 2.06 |
| Ash %  | 0.004 |
|   |   |
| **Distillation Vol. recovered** % |   |
| 0 - 200°C | 21.00 |
| 300°C  | 41.00 |
| 350°C  | 50.00 |
| Water and Sediments, Max | 1.2 |
|  |  |
| **REBCO (GOST 9965-76)** |
| Maximum Sulfur Content 1,8% Paraffin Content 6,0%Maximum Water & Sediment Content 1,2%Distillation, Weight 21%Up to 200° Ñ min 21Up to 300° Ñ min 41Up to 350° Ñ min 50Maximum salts content, MG/L 100 |